# *Evidences Configuration Help*

***Use Evidences Toolkit***

*Defines wether the Evidences Toolkit should be used. If not, no evidences will be generated by the domibusConnector at all.*

***Hash algorithm***

*With the SubmissionAcceptenceEvicence the main document (PDF) of the message will be attached for reliability. This document will be attached as a hashed value. The algorithm defines how this hash value is generated. Possible values are MD5, SHA1 and SHA256.*

***Use Evidences Timeout***

*Defines wether the Evidences Timeout should be used. If not, the domibusConnector will not follow the reception of evidences to outgoing messages.*

**Timeout for RelayREMMD evidences (ms)**

*Defines the timeout for RelayREMMD evidence to be sent back when an outgoing message was sent.*

*After this period, if an outgoing message was sent to the gateway successfully and no RelayREMMD evidence was received, a RelayREMMDRejection will be created for this message and sent back to the national system.*

*Value is in milliseconds. For seconds divide value with 1000. For hours divide value with 3600000.*

**Timeout for Delivery evidences (ms)**

*Defines the timeout for Delivery evidence to be sent back when an outgoing message was sent.*

*After this period, if an outgoing message was sent to the gateway successfully and no Delivery evidence was received, a NonDelivery evidence will be created for this message and sent back to the national system.*

*Value is in milliseconds. For seconds divide value with 1000. For hours divide value with 3600000.*

**Timeout for Retrieval evidences (ms)**

*Defines the timeout for Retrieval evidence to be sent back when an outgoing message was sent.*

*After this period, if an outgoing message was sent to the gateway successfully and no Retrieval evidence was received, a NonRetrieval evidence will be created for this message and sent back to the national system.*

*Value is in milliseconds. For seconds divide value with 1000. For hours divide value with 3600000.*

## *****Configuration of address for evidences generating:*****

*When the SubmissionAcceptanceEvidence is generated, this address will be added to the evidence. This is due to the ETSI-REM standard.*